Obrázek

PRICE OFFER

TABLE SAW

MODEL: SPEED FORMAT

Obrázek



Obrázek

|  |  |
| --- | --- |
| KLIENT: | |
| Názov spoločnosti: |  |
| Adresa: |  |
| IČ DPH: |  |
| Kontaktná osoba: |  |
| Mena ponuky: | Euro |
| Dátum ponuky: | 2022 / 2023 |

1. **BASIC DESCRIPTION OF THE MACHINE**

Professional table saw for longitudinal cuts.

The machine is an ideal solution for all companies whose priority is the processing of solid wood. The machine has no tilt or precut. It offers a robust and stable construction with a large number of configurations.

**Basic division of the machine:**

|  |  |  |
| --- | --- | --- |
| **Type** | **BASIC** | **TOP** |
| **Type of electric fence** | Standard 5 memories | Programmable with touch screen |
| **Extension tables** | - | 1x central sliding  1x rear  1x table behind the cut |
| **Laser** | - | YES |
| **Foot cut trigger** | Button operation / Optional small foot switch | Full-length foot control |

**Version of the parallel fence:**

1. **Basic, electrically adjustable with numerical positioning and memory containing 5 values**



1. **Programmable fence - Control using a PLC and touch display.**
2. **Extended fence with grippers for processing flat materials and glulam panels with the possibility of cutting into strips. Length 1000 - 3200mm**
3. TECHNICAL PARAMETERS OF THE MACHINE

|  |  |
| --- | --- |
| Machine model | Speed Format 6200 |
| Maximum saw blade diameter | ø 550 / 30 mm |
| Number of reel blade positions | 60 / 100 / 160 mm |
| Maximum cutting height with a 550mm disc | 160 mm |
| Tilting of the saw aggregate | NO |
| Speed of the main saw blade | 3500 rpm. |
| Main engine power | 5.5 / 7.5 / 11 kW |
| Cut with a standard parallel fence | 500 mm |
| Table size | 6200 × 1000 mm |
| Cut length | 6200 mm |
| Cutting speed | 5 – 30 m / min |

1. ADDITIONAL EQUIPMENT

|  |  |
| --- | --- |
| Additional equipment | |
| Additional ruler stopper | 45 euro / pc |
| Central cross table + fence ( moveable ) | 2500 euro |
| End cross table + fence ( static ) | 1500 euro |
| Extending the cut with a parallel fence | + 500 mm = + 750 euro |
| Excentric pressure on ruller | 150 euro |
| Laser for marking the cut | 500 euro |
| Rear table extension for cross-cutting long materials | 1050 euro |
| Digital cross fence with one stopper | 1 000 euro |
| Extended fence with pneumatic gripper + PLC control and touch screen display | L2000= 10 000 euro |
| Programming fence with touch screen display | 5 000 euro |
| Main engine power 11kW | 800 euro |
| Small foot switch | 700 euro |
| Full-length foot control | 2000 euro |
| Individual changes to the machine are possible by agreement |  |
|  |  |

1. PRICE OFFER AND PAYMENT TERMS:

|  |  |
| --- | --- |
| Offer | |
| Machine | SPEED FORMAT 4200 7.5kW / BASIC |
| Validity of the offer: | 30 Days |
| Delivery date | 8-12 Weeks |
| Terms of payment: | 30% Before production / 70% before expedition |
| Warranty: | 12 months |
| Price offer: | 29 000 euro without VAT |
| Price for machine | 29 000 euro |


|  |  |
| --- | --- |
| Machine alternatives | |
| SPEED FORMAT 3200 7,5kW / BASIC | 21 000 euro |
| SPEED FORMAT 4200 7,5kW / BASIC | 23 000 euro |
| SPEED FORMAT 5200 7,5kW / BASIC | 26 000 euro |

|  |  |
| --- | --- |
| BASIC configuration | |
| Machine | SPEED FORMAT 6200 / 7.5kW / BAISC |
| Central cross table | - |
| Laser | - |
| Width of cut | 500 mm |
| Electric ruler ( „2“ ) | Memory with 5 values |
| Engine | 7.5 |
| Rear table extension for cross-cutting long materials | - |
| SUMAR PRICE | 29 000 |

|  |  |
| --- | --- |
| Machine alternatives | |
| SPEED FORMAT 4200 7,5kW / TOP | 31 000 euro |
| SPEED FORMAT 6200 7,5kW / TOP | 38 000 euro |

**Suitable to the machine**

**SPS – 500**

****

**Machine description:**

Fully electric bottom shortening saw KUSING SPS-500 with the power of the main motor 3, 4, 5.5kW.

Continuously adjusting the speed of the cutting cycle using a frequency converter from 2 to 6 s.

The machine is produced in two versions ("A" "B") when the position of the ruler relative to the axis of the disk changes, which makes it possible to adjust the parameters of the cross-section.

Cross-section of variant "A": 50 x 300 / 150 x 200

Section "B" variant: 50 x 350 / 120 x 300

**Technical parameters:**

Max. material width: 300 / 350 mm

Max. Material thickness: 150 mm

Shaft diameter: 30 mm

Saw blade diameter: 500 mm

Saw blade speed: 3500 rpm.

Engine power: 3 / 4 / 5.5 kW

Power motor: 0.55 kW.



Cutting cycle speed with FM: 2-6 s. / cycle.

Weight of the machine approx.: approx. 280 kg


Suction: 1 x 120 mm.

Machine dimensions: W / L: 1100 x 800 mm

Working height: 860 mm

** **

**Variant „A“ Variant „B“**

****

**Rulers according to the request: price: 100 euro / m**

**Mechanical stopper on the ruler: 45 euro / pc**

**Penumatic stopper: 450 euro / pcs.**

**Option of controlled ruler according to specification**

**Roller tracks according to specification**

4. **CONCLUSION:**

Dear business partners,

KUSING is a manufacturer of woodworking machines with a tradition dating back to 1991. It is a traditional manufacturer of woodworking machines with its own production technology.

With our products, you are not only buying a machine, but also the assurance that we will take care of your machine in full throughout the machine's lifetime, including all spare parts and later service.

Our service technicians are at your disposal 24/7, whether it is quick advice on the delivery of the machine.

Thank you for your interest in our services and the trust you have shown.

We wish you a nice day.

Sincerely, KUSING Collective.

For more information, call: Ján Kurila +421 948 330 442